;****************************************************************************
;****************************************************************************
;**             (C)Copyright 1987-2020, TYAN COMPUTER CORP.                **
;**                                                                        **
;**                      http://www.tyan.com                               **
;**                                                                        **
;**                                                                        **
;****************************************************************************
;****************************************************************************

S5630 Firmware Release Note
=============================================================================
V7.00	- Date	 : 01/09/2020
	- Filename   : 5630010700.ima
	- Checksum   : 3F3CD3B6<CheckSum32>
	- Description:
		-- Based on 56300105.ima
		-- Add force change password at first time login successfully. 
                   It includes IPMI, WebUI and Redfish.
                   Requires user to update the BMC password upon first login to 
                   comply with California Senate Bill 327 (SB-327)
		-- Support Redfish 1.5
		-- Improve Web performance on Dashboard / SEL and sensor polling
		-- Security Update: Update JAVA signing key
		-- Support stronger SSL ciphers to fix the security issue is reported by OpenVAS utility.
		-- Pop up a message after flashing BIOS via Web successfully
		-- Fix upload and generate SSL certificate issue
		-- Fix unable to flash BIOS via TFTP
		-- Add PSU FRU support
		-- Add Pwr Unit Status sensor(D8h) and IPMI Power control sensor(D9h~DEh)
		-- Add SPS FW Health(17h)/NM Exception(18h)/NM Health(19h) and NM Threshold Exceeded(1Bh) event sensor
		-- Mounting folder support in JViewer
		-- Support trigger status LED when discrete sensor report error
		-- Relax the validation rule while setting domain name on DNS Configuration page
			ex: us-or.whitebox.equipment
                -- Set Green Well default To Disable
		-- Set Entity Instance of CPU related sensors start from 1
                -- Support Greenwell Enable/Disable command
                -- Support PCIE Device ID Command
                -- Support set T_high command
	-- Known issue:
       	1. Redfish Password cannot be reset to default  after restore factory setting.
		2. There is no option to preserve redfish configuration.
	
	*Note: Please follow the update process to update BMC FW first then program 
           the new BIOS with Redfish enabled.

=============================================================================

  
	   
