	                   BIOS Engineer Release Note

;**********************************************************************************
;**********************************************************************************
;**									   	 **
;**		   (C)Copyright 1987-2020, TYAN COMPUTER CORP.         	   	 **
;**									   	 **
;**			      All Rights Reserved.			   	 **
;**									   	 **
;;**									  	 **
;**********************************************************************************
;**********************************************************************************

[]========================<< Released >>===========================[]
V2.02                - Date : 03/18/2020
	        - Filename : 5630V202.ROM
	        - CheckSum : E77F<h>
                        - MD5: 768d48caf6a9ad417e6eeac23b3d29da
                       
	        - Intel RC : Central Park Purley-R Release RC0595.D04(IPU 2019.2)
                        - MicroCode: MB750654_02000069.mcb (Skylake ,stepping H-0,M-0,U-0)
                                              MB750655_03000012.mcb (Cascade,stepping A-0)
                                              MBF50656_04002F00.mcb (Cascade,stepping B-0)
                                              MBF50657_05002F00.mcb (Cascade,stepping B-1)
	        - Intel ME : SPS_E5_04.01.04.381.0( NodeManager )
	        - AMI label: 5.14_PurleyCrb_0ACLA049
	        - Recovery : 5630_001.CAP
                - VGA OpROM : V1.09.00
	        - Banner   : TYAN S5630 Server BIOS V2.02
	        - Description
                                        - Update sps to SPS_E5_04.01.04.381.0.(Mitigate CVE-2020-0545 vulnerability)
                                        - Update microcode(H0/B0/B1) to ver 69/2F00/2F00.
                                        - Solve issue that smbios UUID sync fail.
                                        - Set BMC User Password at least 8 characters.
                                        - Update AMI codebase to 5.14_PurleyCrb_0ACLA049.
                                        - First release to support redfish.

==========================================================================================================




A local flash BIOS with ME update step by step:
               01) Extract 5630XXXX.zip to USB Storage.
               02) Power on your system and boot to EFI SHELL.
               03) Change and find the USB storage current directory (For example 'fs0:\5630XXXX').
               04) Run flash.nsh
               05) If error shows "rom layout change", please use method B to do the flash.
               06) Flash finished, do AC off.
               07) AC on, check BIOS revision and ME revision with normal status on BIOS Setup Menu.


Remote flash bios step by step:
        01) Extract 5630xxxx.xxx to USB Storage.
        02) Connect Lan to the B5630 system's management port 1.
        03) Power on your B5630 system to get the management IP then shut down the system(S5 state).
        04) Use another local NB or PC also connect to the same network with Linux environment.
        05) Change and find the USB storage current directory in the local system.
        06) Run command "ipmitool -I lanplus -H xx.xx.xx.xx -U Administrator -P jumpm3 -b 6 -t 0x2c raw 0x2e 0xdf 0x57 0x01 0x00 0x01"
            then delay a few seconds.
        07) Run command "Yafuflash -d 2 -nw -ip xx.xx.xx.xx -u root -p superuser 5630xxxx.xxx".
            wait for bios flash completed.
        08) Run command "ipmitool -I lanplus -H xx.xx.xx.xx -U Administrator -P jumpm3 -b 6 -t 0x2c raw 0x2e 0xdf 0x57 0x01 0x00 0x02"
            then delay a few seconds.
        09) Do B5630 system on.
        10) Check BIOS revision and ME revision with normal status on BIOS Setup Menu.


